/interface wireless security-profiles

set [ find default=yes ] authentication-types="" eap-methods=passthrough \

    group-ciphers=aes-ccm group-key-update=5m interim-update=0s \

    management-protection=disabled management-protection-key="" mode=none \

    name=default radius-eap-accounting=no radius-mac-accounting=no \

    radius-mac-authentication=no radius-mac-caching=disabled \

    radius-mac-format=XX:XX:XX:XX:XX:XX radius-mac-mode=as-username \

    static-algo-0=none static-algo-1=none static-algo-2=none static-algo-3=\

    none static-key-0="" static-key-1="" static-key-2="" static-key-3="" \

    static-sta-private-algo=none static-sta-private-key="" \

    static-transmit-key=key-0 supplicant-identity=MikroTik tls-certificate=\

    none tls-mode=no-certificates unicast-ciphers=aes-ccm wpa-pre-shared-key=\

    "" wpa2-pre-shared-key=""

/interface wireless

set 0 adaptive-noise-immunity=ap-and-client-mode allow-sharedkey=no \

    antenna-gain=0 area="" arp=enabled band=2ghz-b/g basic-rates-a/g=6Mbps \

    basic-rates-b="" bridge-mode=enabled channel-width=20mhz compression=no \

    country=no_country_set default-ap-tx-limit=0 default-authentication=yes \

    default-client-tx-limit=0 default-forwarding=no dfs-mode=none \

    disable-running-check=no disabled=no disconnect-timeout=3s distance=\

    dynamic frame-lifetime=0 frequency=2437 frequency-mode=manual-txpower \

    frequency-offset=0 hide-ssid=no ht-ampdu-priorities=0 ht-amsdu-limit=8192 \

    ht-amsdu-threshold=8192 ht-basic-mcs=\

    mcs-0,mcs-1,mcs-2,mcs-3,mcs-4,mcs-5,mcs-6,mcs-7 ht-guard-interval=any \

    ht-rxchains=0 ht-supported-mcs="mcs-0,mcs-1,mcs-2,mcs-3,mcs-4,mcs-5,mcs-6,\

    mcs-7,mcs-8,mcs-9,mcs-10,mcs-11,mcs-12,mcs-13,mcs-14,mcs-15,mcs-16,mcs-17,\

    mcs-18,mcs-19,mcs-20,mcs-21,mcs-22,mcs-23" ht-txchains=0 \

    hw-fragmentation-threshold=disabled hw-protection-mode=none \

    hw-protection-threshold=0 hw-retries=7 l2mtu=2290 mac-address=\

    D4:CA:6D:7B:08:63 max-station-count=2007 mode=ap-bridge mtu=1500 \

    multicast-helper=default name=wlan1 noise-floor-threshold=default \

    nv2-cell-radius=30 nv2-noise-floor-offset=default nv2-preshared-key="" \

    nv2-qos=default nv2-queue-count=2 nv2-security=disabled \

    on-fail-retry-time=100ms periodic-calibration=enabled \

    periodic-calibration-interval=10 preamble-mode=both \

    proprietary-extensions=post-2.9.25 radio-name=D4CA6D7B0863 \

    rate-selection=advanced rate-set=configured scan-list=default \

    security-profile=default ssid=DMZona.ru station-bridge-clone-mac=\

    00:00:00:00:00:00 supported-rates-a/g=\

    6Mbps,9Mbps,12Mbps,18Mbps,24Mbps,36Mbps,48Mbps,54Mbps supported-rates-b=\

    "" tdma-period-size=2 tx-power=24 tx-power-mode=card-rates \

    update-stats-interval=disabled wds-cost-range=50-150 wds-default-bridge=\

    none wds-default-cost=100 wds-ignore-ssid=no wds-mode=disabled \

    wireless-protocol=unspecified wmm-support=disabled

/interface wireless manual-tx-power-table

set wlan1 manual-tx-powers="1Mbps:28,2Mbps:28,5.5Mbps:28,11Mbps:27,6Mbps:28,9M\

    bps:27,12Mbps:27,18Mbps:26,24Mbps:24,36Mbps:23,48Mbps:23,54Mbps:22,HT20-0:\

    17,HT20-1:17,HT20-2:17,HT20-3:17,HT20-4:17,HT20-5:17,HT20-6:17,HT20-7:17,H\

    T40-0:17,HT40-1:17,HT40-2:17,HT40-3:17,HT40-4:17,HT40-5:17,HT40-6:17,HT40-\

    7:17"

/interface wireless nstreme

set wlan1 disable-csma=no enable-nstreme=no enable-polling=no framer-limit=\

    3200 framer-policy=none

/interface wireless align

set active-mode=yes audio-max=-20 audio-min=-100 audio-monitor=\

    00:00:00:00:00:00 filter-mac=00:00:00:00:00:00 frame-size=300 \

    frames-per-second=25 receive-all=no ssid-all=no

/interface wireless sniffer

set channel-time=200ms file-limit=10 file-name="" memory-limit=10 \

    multiple-channels=no only-headers=no receive-errors=no streaming-enabled=\

    no streaming-max-rate=0 streaming-server=0.0.0.0

/interface wireless snooper

set channel-time=200ms multiple-channels=yes receive-errors=no

