# oct/17/2018 16:39:23 by RouterOS 6.43.2
# software id = EI26-VVL9
#
# model = RouterBOARD cAP 2nD
# serial number = 8D5E08A118B9
/interface bridge
add admin-mac=CC:2D:E0:E3:4C:55 auto-mac=no comment=defconf name=bridge
/interface wireless
# managed by CAPsMAN
# channel: 2412/20-Ce/gn(20dBm), SSID: IB, CAPsMAN forwarding
set [ find default-name=wlan1 ] band=2ghz-b/g/n channel-width=20/40mhz-Ce \
    distance=indoors frequency=auto mode=ap-bridge ssid=MikroTik-E34C56 \
    wireless-protocol=802.11
/interface ethernet
set [ find default-name=ether1 ] advertise=\
    10M-half,10M-full,100M-half,100M-full,1000M-half,1000M-full
/interface wireless security-profiles
set [ find default=yes ] supplicant-identity=MikroTik
/ip hotspot profile
set [ find default=yes ] html-directory=flash/hotspot
/interface bridge port
add bridge=bridge comment=defconf hw=no interface=ether1
add bridge=bridge comment=defconf interface=wlan1
/interface wireless cap
# 
set discovery-interfaces=ether1 enabled=yes interfaces=wlan1
/ip dhcp-client
add comment=defconf dhcp-options=hostname,clientid disabled=no interface=\
    bridge
/ip service
set telnet disabled=yes
set ftp disabled=yes
set ssh disabled=yes
set api disabled=yes
set api-ssl disabled=yes
/system clock
set time-zone-name=Asia/Krasnoyarsk
/system identity
set name=123
/system routerboard settings
set silent-boot=no
