admin@MikroTik] > export
# jan/02/2019 06:08:32 by RouterOS 6.42.6
# software id = 7J7G-GK80
#
# model = 411U
# serial number = 3DA20296EE04
/interface ethernet
set [ find default-name=ether1 ] name=LAN_ok
/interface list
add name=WAN
add name=LAN
/interface wireless security-profiles
set [ find default=yes ] supplicant-identity=MikroTik
/port
set 1 name=usb2
/interface ppp-client
add apn=ogcs data-channel=1 dial-on-demand=no disabled=no info-channel=2 \
    modem-init="AT+CFUN=1" name=LTE phone=*99# port=usb2
/interface bridge port
add interface=LAN_ok
add interface=all
/interface bridge settings
set use-ip-firewall=yes
/interface list member
add interface=LAN_ok list=WAN
/ip address
add address=192.168.88.1/24 comment=defconf interface=LAN_ok network=\
    192.168.88.0
add address=192.168.0.66/24 comment=Lan2 interface=LAN_ok network=192.168.0.0
/ip firewall nat
add action=masquerade chain=srcnat out-interface=LTE
/system identity
set name=MikroTik
/system routerboard settings
[bookmark: _GoBack]set silent-boot=no
